Employee of Facilities and Services (F&S) may participate in inspections, assessments, investigations or use GPS data collection equipment on construction sites. At a minimum, these employees should wear:

* Shirt with sleeves (short-sleeve is fine; no sleeveless shirts or tanks),
* Long pants, and
* Closed toe shoes.

Additional PPE will likely be required depending on the hazards associated with the specific project, such as:

* Safety glasses
  + Provide protection from flying objects.
  + Must be stamped with ANSI Z87.1 to be considered safety glasses.
* Hard hat
  + Provide protection from falling objects and reduce electrical shock hazards when near exposed electrical conductors which could contact the head.
* High visibility apparel
  + When working in and around vehicular traffic and construction equipment.
  + High visibility apparel allows the user to be distinguished from the surrounding environment.
  + ANSI Class 3 high visibility apparel is recommended.
* Hearing protection
  + As a general rule, if you are an arm’s length away and have to raise your voice to communicate, you should be wearing hearing protection.
* Protective footwear
  + Provides protection against falling or rolling objects, or objects piercing the sole.
  + If a job requires protective safety footwear, F & S employees are eligible for partial reimbursement of ASTM/ANSI approved safety footwear.

Safety glasses, hard hats, high visibility vests, and hearing protection can be checked out at the F & S Tool Room.

The jobsite coordinating contractor has the latitude to specify additional PPE.